Subsections

- - Scopes:
  - Settings:
  - Sliders:
- Waveform/RGB Parade/Waveform Ply
- Adjusting luminance
- HDTV or sRGB (ITU-R BT.709)
- MPEG or Analog video (ITU-R BT.601)
- NTSC Television broadcast
- Vectorscope
- Histogram

##
Videoscope

Videoscope summarizes intensity and color on a calibrated display. The Videoscope can be used in conjunction with other CINELERRA-GG plugins such as Color 3 Way, YUV, Brightness, Color Balance or Histogram to accurately correct video for contrast, clarity, conformance (to normalize various videos shot under different light settings), or for cinematic purposes. The human eye is not specialized to match precise level of light and color, but Videoscope is. Videoscope contains three displays: the waveform scope and the vectorscope, plus the histograms (figure 10.76). Instead of applying the plugin to the tracks/edits we want to examine, we can use the Videoscope buttons in the Composer and Viewer windows. In this way the monitors act on the frame indicated by the insertion point, without taking into account the stack of tracks or on which edits to apply the plugin.

Figure 10.76: GUI of the Videoscope. You see Histogram, RGB Parade and Vectorscope

If the original source has values outside the range (0 - 1.0f ), the plugin will always produce clipping. The display will stop at -10% or +110%, but there is no clipping. For example, by varying the brightness all out-of-range values become visible on Waveform, even over 110%. However you must disable the "smooth" option which always causes clipping.

The Videoscope menu window has many options.

#### Scopes:

we can choose between two histograms:

- Histogram
- Histogram RGB

three waveforms:

- Waveform
- Waveform RGB (aka RGB Parade)
- Waveform Ply (which superimposes the three Waveform RGB graphs in a single view.)

and two vectorscopes:

- Vectorscope
- VectorWheel

#### Settings:

It is divided into two sections. The upper section contains two items:

Smooth:
  serves to make the graph more homogeneous, improving its visualization. However, it has a side effect: in case of frames that have data in the range of 100-110% (i.e., outside the normal range of 0-100%, also called super-white), it causes a clip by cutting off this data and reporting only of normal data. If we don't want this clip disable Smooth.
Refresh on Stop ON:
  [checked – only for Transport buttons] scopes are updated when you stop playback at a given location. Instead, they are locked at the start position while you playback. This saves system resources and makes playback smoother. By dragging the cursor the scopes are updated in realtime.
Refresh on Stop OFF:
  [unchecked – for Transport buttons and dragging cursor] the display of the scopes is synchronized with the playback. Every variation of the graphs is in realtime. There may be some decrease in fps during playback.
Refresh on Release:
  This works for the Viewer and Compositor windows. Scopes are not updated during playback. The update occurs only when you stop playback, that is at the final position (either by dragging the cursor or using the Transport buttons). When in the timeline, if you drag on the TimeBar or reposition in the TimeBar in either Drag and Drop or Cut and Paste mode, the release of the button also will update the Scopes. This saves system resources and makes playback smoother. Because there is no update when playing in the main window, you can still easily get a videoscope update simply by moving the mouse to the Compositor and a single click there will update the scopes without changing the frame (as long as Click to Play is not enabled).

The lower section, called VectorWheel Grids, it is only active when VectorWheel is set up in Scopes pull-down and contains four entries (figure 10.77):

Figure 10.77: Pull-down Settings

None:
  It only shows the colour wheel, without any superimposed graticula.
All:
  Shows the most complete grid that allows precise and useful measurements. It also shows the skintones area.
Hue:
  Show a more minimal grid. It also shows the I-Line.
IQ:
  Show shows only I-Line and Q-Line.

You can create custom grids. These are raster .png images of adequate resolution and must be put in:

    [your cinelerra path]/bin/plugins/scopes/custom_grid.png

More information in the later section on Vectorscope.

#### Sliders:

allow for varying the solidity of the dots shown in Waveforms and Vectorscope. You can get to the subpixel level for precision. They are accompanied by Reset buttons that restore them to default values.

###
Waveform/RGB Parade/Waveform Ply

The Waveform Scope displays image intensity (luminance) versus image X position. The Waveform RGB displays image RGB intensity versus image X position (one graph per channel). The Waveform Ply shows the three channels in a single graph. The Waveform Scope appears on the left side or in the middle of the Videoscope window. The display is calibrated vertically from 0% intensity (black) at the bottom up to 100% intensity (white) at the top. Each column of pixels in the image corresponds to one column of pixels in the Waveform Scope (figure 10.78). Note that the height of the values of a waveform/waveform RGB corresponds exactly to the values on the x axis in the histogram. A vertical/horizontal correspondence is therefore obtained.

Figure 10.78: Colortest 75% with Waveform RGB (left) and Waveform (right)

On the left is shown waveform RGB: instead of the color shadows as in figure 10.76, we have lines representing the color bar test at 75%. They are pure colors, so all pixels have the same value. In fact, they are all at the level of 75% except for the 100% white band and the 0% black band. In the waveform on the right, we have the same behavior with regard to luminance: the white band is 100%; the black band is 0% and all the others 75%.

If we left-click on the graph with the mouse, we will see a crosshair that we can place exactly where we want to measure. We can read the precise values of X and Luminance (Value) in the pop-up box that appears at the bottom right (figure 10.79).

Figure 10.79: Examples of waveform (with crosshair and the coordinates' box), waveform RGB and waveform Ply

The Waveform scope helps correct image light levels for contrast range or for conforming light levels on various scenes originally shot on different light settings. The same can be done with Waveform RGB or the convenient overlapping representation (Waveform Ply).

###
Adjusting luminance

1. Add the Brightness/Contrast, Histogram, Color 3 Way or another video adjustment effect on your track/edit.
2. Add the Videoscope effect on the track. Make sure that it is placed below in the stack of effects, so it can see the adjustment effect's results. If it is not, right-click and move it down. Or do not use the plugin but activate the Videoscope button in the Compositor window.
3. Show both the effect and Videoscope.
4. Adjust the contrast while observing the waveform to match the desired light level.
5. Precise adjustments can be made by measuring the values on the waveform with the crosshair (by clicking LMB, and reading numeric values on the pop-up box) and reporting these numbers in the effects window (Histogram Bézier, for example).

For example, if you are looking for maximum contrast range, adjust the Brightness/Contrast levels to align the darkest point on the scope with the 0% level and the brightest portion with 100%. Anything above 100% is over saturated. Limits may be highlighted with checkbox controls.

###
HDTV or sRGB (ITU-R BT.709)

The maximum pixel range for HDTV or sRGB is [0, 255]. This range corresponds with levels 0% and 100%.

###
MPEG or Analog video (ITU-R BT.601)

For analog video or MPEG (including DVD), the maximum range for RGB is [16, 235] (8 bit). For YUV, the maximum range for intensity (Y) is [16, 235] (8 bit). This range corresponds to gray levels from 6% to 92%. Reference RGB-601 plugin.

###
NTSC Television broadcast

If you are producing a video for NTSC television broadcast, keep the intensity between 7.5% and 100%. The minimum black value which can be broadcast is IRE 7.5% (indicated by the 7.5 level), and values below this level are no darker.

###
Vectorscope

The Vectorscope displays hue (angle on the color wheel) and saturation (radius). Each pixel in the source image is drawn as a point on the color wheel. The distance from the center is the color saturation. Gray values are close to the center, and high saturation values are near the perimeter (100%). In the center there is pure white (0%). By clicking with the mouse on the color wheel a radius and circle will appear whose values of hue and saturation are shown in the pop-up box at the bottom right of the window, similar to the values of X and luminance of the Waveform and RGB Parade (figure 10.80).

Figure 10.80: Vectorscope (with H/S pop-up box) and VectorWheel (with 3 default grids)

Note that when you choose VectorWheel from Scopes pulldown, you can choose between different grids in the Settings pulldown. In addition, any number of user-supplied grid patterns can be added in the form of a square image of type png. The user can design and maintain individual grid overlays for various purposes. The user would keep their overlays in a safe spot on their disk and make a copy of them in the {cinelerra_pathname}/bin /plugins/scopes every time a new version of CINELERRA-GG is installed.

Generally the Vectorscope has the following uses:

1. Compare saturation levels (radius) between Edits.
2. Compare the hues (angle) between Edits.
3. Compare skin tones, sky and vegetation.
4. Display the color balance or color cast.
5. Check the legal limits of the video signal.

For example, skin tones are found along an axis (+ I-line) between yellow and red, and between 0 and 50% saturation values. The blue of the sky is more or less along the opposite axis to that of the skin (- I-line), with a much wider saturation range.

Figure 10.81: Balancing a yellow color cast

In figure 10.81, the top image is white balanced. Vectorscope shows many pixels in the yellow region and few in the white region. To remove the yellow tint, the Color Balance effect is used to first shift the vectorscope plot towards magenta (Mg), and then towards blue (B) until the region previously near the center surrounds the center. In the bottom image, yellow highlights have become white highlights (green triangles). Note that the corresponding features in waveform also appear whiter (green triangles). The Vectorscope can also be used to verify that the video output will display properly on various monitors. Any points along the inner radius will be displayed as pure white and any points above the 100% radius, will probably not be correctly displayed on the screen.

###
Histogram

You can also display the 4 histograms (master or RGB) on the left of the window. (see figure 10.76).